**General Information: MAIN STAGE**

**Contact Address:** Burnley Mechanics Theatre

Burnley Leisure Trust

Manchester Road

Burnley

Lancashire BB11 1BH Dock Door Sat Nav: BB11 1HD

**Telephone Nos.:** Administration (all depts.): 01282 477114

Box Office: 01282 664400

**Technical Contacts:** Technical Manager Sam Leahy 01282 664400 ext. 3215 (Office)

[sleahy@blcgroup.co.uk](mailto:sleahy@blcgroup.co.uk)

Chief Technician Angus Allan 07496969706 (Mobile)

[aallan@blcgroup.co.uk](mailto:aallan@blcgroup.co.uk)

**Parking:** From Yorke Street, turn left into the car park through the yellow gates.

The Loading Bay is on the left, behind the Basement Studio.

We can accommodate a 13.7m/45’ truck and a tourbus, although prior

notice is required to ensure space is available.

16amp power for trucks and buses by prior arrangement.

**N.B. This area is patrolled by Civil Enforcement Officers.**

Please ensure that you obtain a valid parking permit from a member

of theatre staff, as we cannot be held responsible for vehicles being

ticketed for not displaying one.

**Get-In:** Access to the theatre, which is situated on the third floor, is via

a goods lift.

The lift dimensions are 2.6m (l) x 1.6m (w) x 2.3m (h).

Maximum weight capacity is 2250kg.

Any items that are too large for the lift can be brought in via the

main entrance or, if suitable, hoisted up the outside of the building

via a 500kg hoist (weather permitting).

Once at theatre level there is a tail lift to access the dock doors, with

a maximum weight capacity of 1000kg.

**Auditorium:**

**Capacity:**  Tiered Seating 370

Stalls Seating 123

Total 493

Standing Event 700

The seating is fully configurable to suit your event, and can include

a flat floor performance area, cabaret style seating, full banquet

seating, etc.

**Control Room:** Located at the back of the auditorium, behind the tiered seating.

Removable windows at both LX and Sound positions.

**FOH Positions:** In addition to the Control Room, FOH positions are available at

the bottom, middle and top of the tiered seating (outside the

Control Room). All positions are off-centre.

**All these positions require the removal of seating and therefore**

**must be reserved at time of booking with the Technical Manager.**

**Stage:**

**Construction:** Wooden. Oil-resistant hardboard over 1” ply.

Painted matt black. Not raked.

Solid white Cyc with black tabs in front.

Black legs (4) and hard masking (4) available.

Access is via dock doors SL.

Wing space and storage space SL. No wings SR.

**Dimensions:** Stage Depth 8.5m – this includes permanent stage extension

10m (w) x 1m (d).

Stage Width 9.5m

Pros. Width 8.5m

Pros. Height 4.0m

Truss Height 5.5m

**Prompt/SM:** DSL. Show relay and call facilities to FOH and dressing rooms.

TV monitor of FOH stage view.

**Flying:** Half-height flying (apex roof).

15 x 9m long hemps sets, rated at 25kg per set.

**Curtains:** Red house tabs, controlled form Stage or Control Room.

Black halfway tabs, manually operated from SL.

Safety curtain behind Pros. – must be kept clear.

**Crossover:** There is no onstage crossover.

Access to SR is via several flights of stairs.

**Piano:** Steinway C Grand Piano available on request – this is not

located on stage, must be booked in advance.

*\*Hire and tuning charges apply\**

**Dressing Rooms:**

**Location:** All dressing rooms are located on the floor above the stage,

Accessed by stairs SL.

**Description:** Dressing Room 1 10 persons

Dressing Room 2/3 6/4 persons – can be split

Dressing Room 4 5 persons

Dressing Room 5 3 persons

**Facilities:** Rooms 1 – 4 have basins, mirrors, rails, chairs, heating and A/C.

Room 5 has mirrors, a rail and heating.

Rooms 1 and 3 have fridges.

Toilets and showers available.

Laundry and ironing facilities available on request.

**Sound:**

**Mixer:** Soundcraft Expression 3 32-Channel Digital Desk

DBX 260 Speaker Management System

DBX Dual 31-Band Graphic EQ

32 Send/12 Return Analogue Tie-Lines (Split SL/SR)

4 Cat5 Digital Tie-Lines (2 SL/2 SR)

32 Channel Digital Stage Box

**House PA:** Kling & Freitag 12/Horn Top Boxes (4)

Kling & Freitag 6/Horn Delays (2)

Kling & Freitag 6/Horn Front Fills (4)

TP 218 Subwoofers (2)

Achat 206 side fills (fixed position) (4)

Crown XLS 2502 Amplifiers (4)

Total Power 3.5Kw per side

**Additional PA:** Achat 112A 700w Powered Mid/High Boxes (4)

TP 218 Subwoofers (4)

Total Power 6Kw per side

*\*Additional charges apply\**

**Monitors:** EV ELX 12P 1000w powered monitors (5)

TheBox Pro A12 700w powered monitors (2)

EV ELX 18P 700w powered subwoofer (2)

*\*Additional charges apply\**

**Microphones:** A comprehensive selection, including wireless (4)

*\*Additional charges apply\**

**Power Supply:** 63Amp Single Phase (clean) DSL

32Amp Single Phase (clean) DSR, USL, USR

**Lighting:**

**Control:** Chamsys MQ70 Lighting Desk with external Touchscreen

8 Universe ArtNet Distribution System

MagicHD Media Server

MagicVis Visualisation

**Dimming:** ETC Sensor Racks 120 Dimming, 20 Switched

**Rigging:** Adv.1 Truss 8m Box Truss 2 x 250kg Manual Hoists

Adv.2 Truss 6m Tri Truss 2 x 250kg Manual Hoists

Truss 1 8m Box Truss 2 x 500kg Electric Hoists

Truss 2 9m Box Truss 2 x 500kg Electric Hoists

Truss 3 9m Box Truss 2 x 500kg Electric Hoists

Truss 4 8m Box Truss 2 x 500kg Electric Hoists

All trusses have 16Amp hot power and DMX.

See Stage Plan for positions.

**Intelligent Fixtures:** We are mainly a Moving Head house, with the following fixtures:

RGBW Par Cans (20) Various locations on stage

RGBW Cyc Floods (6) Truss 4

Robe LED Wash 300 (8) Truss 1 & 2

Robe Classic 300 Spot (7) Truss 1 & 2

Shark Zoom Wash (18) Truss 3 & 4

MH-200 Spot (12) Truss 3 & 4

Elumen8 LED Profile (14) FOH

MH- z1915 Zoom Wash (5) Adv. 1

Clay Paky 400 Profile (6) Adv. 1

Clay Paky 400 Spot (4) Adv. 2

**FX:** Blinders – 2-Cell (4) and 4-Cell (2)

DMX Sunstrips – White (8) and Coloured (4)

CO2 Coloured Jets (4)

Hazers (2)

Mirror Ball 1m (1)

Starcloth 8m x 4m (2)

*\*Additional charges and fluid cost apply to all FX items\**

**Generics:** We have a small selection of generics, including:

1Kw PC (8), Prelude 16/30 (6)

*\*Additional charges apply to all generics including a fuel levy\**

**Followspots:** Robert Juliat Manon 1200w (2)

*\*Hire and Operator charges apply\**

**The house left followspot requires seats X26 & X27 to be withheld**

**from sale.**

**Power Supply:** 125Amp and 63Amp Three Phase DSL

63Amp and 32Amp Single Phase DSL

**Video:**

**Projector:** NEC 7,200 Lumens

Projector is mounted just in front of Pros.

Hard wired to DSL and Control Room

VGA and HDMI

Remote control shutter

**Screen:** Projects onto White Cyc.

Image size 6m x 4.5m approx.

**Software:** Chamsys MagicHD Media Server

***Please Note: \*Additional charges apply to all asterisked items\****

***All equipment is subject to wear and tear, and possible damage.***

***We endeavour to maintain all our equipment in a serviceable condition, but it is possible that some items may not be available when you visit.***

***Should a particular item be essential for your production, we suggest you inform the Technical Manager at the earliest opportunity.***

***All electrical equipment brought onto the premises MUST have a valid PAT sticker or certification, otherwise we reserve the right to prohibit its use.***

**Directions:**

Travelling East-bound on the M65:

Leave the M65 at Junction 10. Look for the brown sign to Townley Hall.

At the roundabout take the 5th exit onto Cavalry Way. Passing over the

motorway, take the 1st exit from the roundabout, signed Burnley Town Centre.

Take the right-hand lane, and at the traffic lights take the right fork, following

the brown Townley Hall and Burnley Mechanics sign.

You are now on Trafalgar Street. Pass a garage on the left, and a McDonalds and

KFC through the lights on the right.

At the next roundabout, take the first exit towards Town Centre and Mechanics.

Proceed down the hill through the traffic lights, and you will see the Town Hall

on your left (with clock tower).

Burnley Mechanics is on your left immediately after the Town Hall. Turn left

after the Mechanics onto Yorke Street. Left at the bottom and into our Car Park.

Travelling West-bound on the M65:

Leave the M65 at Junction 10. Stay in the left-hand lane on the slip road.

At the roundabout take the 1st exit, signed Burnley Town Centre.

Take the right-hand lane, and at the traffic lights take the right fork, following

the brown Townley Hall and Burnley Mechanics sign.

You are now on Trafalgar Street. Pass a garage on the left, and a McDonalds and

KFC through the lights on the right.

At the next roundabout, take the first exit towards Town Centre and Mechanics.

Proceed down the hill through the traffic lights, and you will see the Town Hall

on your left (with clock tower).

Burnley Mechanics is on your left immediately after the Town Hall. Turn left

after the Mechanics onto Yorke Street. Left at the bottom and into our Car Park.